tmf854.v1 > SwitchCriteriaEnable_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The SwitchCriteriaEnable_T Simple Type
This attribute restricts the severity of alarms for which switching criteria is enabled. See Enums::PerceivedSeverity in IA.
<ApplicableTo>1:N trail protection</ApplicableTo>
Simple Type SwitchCriteriaEnable_T
SwitchCriteriaEnable_T is union of (string, string).
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (INDETERMINATE | CRITICAL | MAJOR | MINOR | WARNING | CLEARED).

Enumeration | Description
INDETERMINATE |
CRITICAL |
MAJOR |
MINOR |
WARNING |
CLEARED |

XML
-<xsd:simpleType name="SwitchCriteriaEnable_T"> -<xsd:annotation> -<xsd:documentation> This attribute restricts the severity of alarms for which switching criteria is enabled. See Enums::PerceivedSeverity in IA. <ApplicableTo>1:N trail protection</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:union> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI extensions in a minor version. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="INDETERMINATE" /> <xsd:enumeration value="CRITICAL" /> <xsd:enumeration value="MAJOR" /> <xsd:enumeration value="MINOR" /> <xsd:enumeration value="WARNING" /> <xsd:enumeration value="CLEARED" /> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/SwitchCriteriaEnable

Generated by WSDLdoc ©