Class ESwitchData {Analysis}

Documentation
This object is used to respond to queries regarding the current protection switch status of an
equipment protection group.
MTOSI Specific Documentation
This class is applicable to MTOSI. The specific operations and relationships that apply to MTOSI are listed in SD2-11.
For MTOSI, references to "NMS" can be interpreted as "Requesting OS" and references to "EMS" can be interpreted as "Target OS", i.e., the OS that fulfills requests from another OS.
The statements concerning Object Lifecycle, i.e., whether the object can be created by the NMS or EMS, are not particularly meaningful for MTOSI, since MTOSI does not define management systems with fixed roles such as the NMS and EMS entities in MTNM.
Object Lifecycle: Created by EMS.
Object Creation Notification Issued? No
Object Deletion Notification Issued? No
External Documents

SD2-11_IA-SS_Mapping.xls |

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
eProtectionGroupType | ESwitchData | EProtectionGroupType | M_FOR_N
eSwitchReason | ESwitchData | ESwitchReason | NA
additionalInfo | ESwitchData | CIS SequenceOf Structs::AVP | empty list

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | --Not Named-- | ESwitchData | --Not Named-- | EquipmentProtectionGroup
--Not Named-- | --Not Named-- | ESwitchData | protectedE | Equipment
--Not Named-- | --Not Named-- | ESwitchData | switchToE | Equipment