tmf854.v1 > ProtectionType_T LOCATION: file:/xsd/networkResources/GlobalDefinitions.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ProtectionType_T Simple Type
The protection type identifies whether a protection switch is an MS protection switch or an SNCP protection switch. It should be noted that although the term MSP was chosen as the original specific protection scheme to which the related behaviour applied was Multiplex Section Protection, the label is now more generally applied to any 1+1 or 1:N Trail protection scheme.
Simple Type ProtectionType_T
ProtectionType_T is union of (string, string, string).
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`PROP_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (PT_MSP_APS | PT_SNCP).

Enumeration | Description
PT_MSP_APS |
PT_SNCP |

XML
-<xsd:simpleType name="ProtectionType_T"> -<xsd:annotation> <xsd:documentation> The protection type identifies whether a protection switch is an MS protection switch or an SNCP protection switch. It should be noted that although the term MSP was chosen as the original specific protection scheme to which the related behaviour applied was Multiplex Section Protection, the label is now more generally applied to any 1+1 or 1:N Trail protection scheme. </xsd:documentation> </xsd:annotation> -<xsd:union> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="PROP_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="PT_MSP_APS" /> <xsd:enumeration value="PT_SNCP" /> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (2) ProtectionSwitch_T/protectionType SwitchData_T/protectionType

Generated by WSDLdoc ©