Operation void getAllTopologicalLinks (CIS SequenceOf TopologicalLink topologicalLinks = NA), in Class MultiLayerSubnetwork

Documentation
Get the Topological Links between Managed Elements contained within the Subnetwork and their distinguishing information.
For singletons subnetworks, no topologicalLinks will be returned. The EMS should report topological links at the "lowest" layer (i.e. closest to physical) about which it has accurate knowledge.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS cannot support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

topologicalLinks
/* out */ A list of the Topological Links between Managed Elements contained within the Subnetwork.