Operation void getCapabilities (CIS SequenceOf Structs::AVP capabilities), in Class EMS

Documentation
The operation returns the capabilities of the EMS with information whether they are supported or not supported by the EMS (including the connection management modes indicating whether CC sharing, pending SNCs, and termination inclusion are supported; see attached supporting document modesOfOperation for explanation).
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
External Documents

SD1-23_ModesOfOperation.pdf |

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

capabilities
/* out */ A list of capabilities with information whether they are supported or not supported.
(Attribute Name - Value Pair List) (Capability Name - Supported/Unsupported Value Pair List)