Operation void getTP (Name tpName, ConnectionTerminationPoint tp), in Class ManagedElement

Documentation
Get the Termination Point and its associated distinguishing information identified by an NMS-specified name.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when tpName does not reference a termination point object.
3. ENTITY_NOT_FOUND - Raised when tpName references a TP object that does not exist.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

tpName
/* in */ The unique identifier of the Termination Point.
tp
/* out */ The Termination Point identified by the provided name.