This operation can be used to delete top-level topological links as well as intra-subnetwork topological links.

The behaviour of this operation should be the same as if an EMS user were to attempt to delete a topological link (or equivalent operation) at the EMS user interface.
Therefore, the specific conditions under which the deletion is rejected are left to the EMS implementation.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when topologicalLink name do not exist.
5. UNABLE_TO_COMPLY - Raised when the deletion is rejected based on EMS own criteria.
