AcknowledgeIndication acknowledgeIndication = NOT_APPLICABLE, in Class AlarmInformation

Documentation
Defines if the alarm has been acknowledged or not.
In case the EMS does not support acknowledgement for this event or does not support acknowledgement at all NOT_APPLICABLE shall be used.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No