RouteChangeState routeChangeState = NA, in Class SNCRouteChangeData

Documentation
This attribute identifies the current state of the reroute operation.
The route change goes through different stages during a reroute of a SubnetworkConnection. These stages are a part of this notification.
Possible values are:
- "RerouteStarted"
- "RerouteCompleted"
- "RerouteFailed"
- "RouteActivated", raised when the route is successfully activated (with reference to the route actualState).
- "RouteDeactivated", raised when the route is successfully deactivated (with reference to the route actualState).
Readable by NMS? Yes
Writeable by NMS? No
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No