Operation setLogFullAction (CIS CharacterString logFullAction = NA), in Class Log

Documentation
The operation sets which action should be taken when the maximum size of the log has been reached. When a log is full its availability status will change to indicate the log full condition.
If the log's full action is set to "halt", then no new log records will be added and the event will be lost. When log records are deleted the log will leave the log full condition and new log records can be added to the log.
If the log's full action is set to "wrap", then new records will be added overwriting the oldest records contained in the log. When log records are deleted the log will leave the log full condition and new log records will no longer overwrite existing log records in the log.
Operation Exceptions:
1. NOT_IMPLEMENTED - If EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter is incorrectly formed.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
The log follow the requested behaviour when the Log is full.
Semantics

Arguments

logFullAction
/* in */ The requested logFullAction of the log.