tmf854.v1 > AliasNameList_T LOCATION: file:/xsd/networkResources/GlobalDefinitions.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The AliasNameList_T Complex Type
This is the definition of the object attribute that contains the list of aliases for the network entity. The attribute is a name-value list. The name refers to the type of alias (e.g., nativeEMSname) and the value component holds the alias itself

Local elements (3)
  alias alias/aliasName alias/aliasValue

Complex Type AliasNameList_T
The AliasNameList_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> <alias> -Begin All [1...1] <aliasName>AliasName_T</aliasName> [1..1] <aliasValue>AliasValue_T</aliasValue> [1..1] End All </alias> [0..*] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:complexType name="AliasNameList_T"> -<xsd:annotation> <xsd:documentation> This is the definition of the object attribute that contains the list of aliases for the network entity. The attribute is a name-value list. The name refers to the type of alias (e.g., nativeEMSname) and the value component holds the alias itself </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element maxOccurs="unbounded" minOccurs="0" name="alias"> -<xsd:complexType> -<xsd:all> <xsd:element name="aliasName" type="AliasName_T" /> <xsd:element name="aliasValue" type="AliasValue_T" /> </xsd:all> </xsd:complexType> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (4) AliasName_T AliasValue_T string TMF854_Version_T

Used-By
Element (17) Alarm_T/aliasNameList ConnectionTerminationPoint_T/aliasNameList EProtectionGroup_T/aliasNameList Equipment_T/aliasNameList EquipmentHolder_T/aliasNameList FloatingTerminationPoint_T/aliasNameList ManagedElement_T/aliasNameList ManagementDomain_T/aliasNameList MultiLayerSubnetwork_T/aliasNameList OperationsSystem_T/aliasNameList PhysicalTerminationPoint_T/aliasNameList ProtectionGroup_T/aliasNameList SubnetworkConnection_T/aliasNameList TopologicalLink_T/aliasNameList TPPool_T/aliasNameList TransmissionDescriptor_T/aliasNameList VendorObject/aliasNameList

Generated by WSDLdoc ©