This operation sets the owner attribute of the specified object.

If there has been a change in the value of the owner attribute, then the EMS forwards an AVC notification.

Operation Exceptions:
1. NOT_IMPLEMENTED - If EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when objectName is incorrectly formed.
4. ENTITY_NOT_FOUND - Raised when objectName references an object that does not exist.
5. UNABLE_TO_COMPLY - Raised when the owner can not be set for the specified object.
6. NE_COMM_LOSS - Raised when communication to managed element is lost.
