tmf854.v1 > SPRINGNodeId_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The SPRINGNodeId_T Simple Type
The protection SPRING node ID. The SPRINGNodeId is used to identify the managedElement during creation of SNCs. This is needed for BLSRs to identify the ingress and the egress nodes so that they know where to loop around in case of failure. Value can be "0" to "15" (may be any other string that matches the SPRINGNodeId transmission parameter values) or "Unknown".
<ApplicableTo>2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type SPRINGNodeId_T
SPRINGNodeId_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace.

XML
-<xsd:simpleType name="SPRINGNodeId_T"> -<xsd:annotation> -<xsd:documentation> The protection SPRING node ID. The SPRINGNodeId is used to identify the managedElement during creation of SNCs. This is needed for BLSRs to identify the ingress and the egress nodes so that they know where to loop around in case of failure. Value can be "0" to "15" (may be any other string that matches the SPRINGNodeId transmission parameter values) or "Unknown". <ApplicableTo>2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/SPRINGNodeId

Generated by WSDLdoc ©