tmf854.v1 > ProbableCause_T > type
LOCATION: file:/xsd/networkResources/ProbableCauses.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The type Element
This is the probable cause specific value.
Element ProbableCause_T/type : union of (string, string, string, string) [1 .. 1]
The type element cannot have "xsi:nil" as an attribute. The type element in XML instance can be substituted with other elements.

XML Instance
This is the probable cause specific value. <type>union of (string, string, string, string)See XML snippet for more information.</type>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element name="type"> -<xsd:annotation> <xsd:documentation> This is the probable cause specific value. </xsd:documentation> </xsd:annotation> -<xsd:simpleType> -<xsd:union> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI extensions in a minor version. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the vendor specific extensions must start with the prefix "PROP_" </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="PROP_([a-z]|[A-Z]|[0-9]|(_-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI pre-defined probable causes. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="UNIDENTIFIED" /> <xsd:enumeration value="AIS" /> <xsd:enumeration value="AMS" /> <xsd:enumeration value="ATPC_FAIL" /> <xsd:enumeration value="AU-AIS" /> <xsd:enumeration value="BER_SD" /> <xsd:enumeration value="BER_SF" /> <xsd:enumeration value="BLOCKED_FE" /> <xsd:enumeration value="CFG_ABORT" /> <xsd:enumeration value="CFG_ABORT_FE" /> <xsd:enumeration value="DCC_FAILURE" /> <xsd:enumeration value="DEMODULATION_FAIL" /> <xsd:enumeration value="EMS" /> <xsd:enumeration value="EMS_ALM_LOSS" /> <xsd:enumeration value="EMS_LIFECYCLE_LOSS" /> <xsd:enumeration value="EMS_ALM_AND_LIFECYCLE_LOSS" /> <xsd:enumeration value="EQPT" /> <xsd:enumeration value="ENV" /> <xsd:enumeration value="FF" /> <xsd:enumeration value="FOP_APS" /> <xsd:enumeration value="INSUFF_LINKS" /> <xsd:enumeration value="INSUFF_LINKS_FE" /> <xsd:enumeration value="LCD" /> <xsd:enumeration value="LIF" /> <xsd:enumeration value="LOA" /> <xsd:enumeration value="LOC" /> <xsd:enumeration value="LODS" /> <xsd:enumeration value="LOF" /> <xsd:enumeration value="LOM" /> <xsd:enumeration value="LOP" /> <xsd:enumeration value="LOPC" /> <xsd:enumeration value="LOS" /> <xsd:enumeration value="LOTC" /> <xsd:enumeration value="MODULATION_FAIL" /> <xsd:enumeration value="MS-AIS" /> <xsd:enumeration value="OS" /> <xsd:enumeration value="OS_ALM_LOSS" /> <xsd:enumeration value="OS_LIFECYCLE_LOSS" /> <xsd:enumeration value="OS_ALM_AND_LIFECYCLE_LOSS" /> <xsd:enumeration value="OSC-AIS" /> <xsd:enumeration value="OSC_BER_SF" /> <xsd:enumeration value="OSC_FERF" /> <xsd:enumeration value="OSC_LOF" /> <xsd:enumeration value="OSC_LOS" /> <xsd:enumeration value="OSC_SD" /> <xsd:enumeration value="PLM" /> <xsd:enumeration value="RAI" /> <xsd:enumeration value="RX_FAIL" /> <xsd:enumeration value="RX_MIS_CONNECT" /> <xsd:enumeration value="RX_UNUSABLE_FE" /> <xsd:enumeration value="SECURITY_VIOLATION" /> <xsd:enumeration value="SQL" /> <xsd:enumeration value="SSF" /> <xsd:enumeration value="STARTUP_FE" /> <xsd:enumeration value="TCF" /> <xsd:enumeration value="TCFE" /> <xsd:enumeration value="TCFI" /> <xsd:enumeration value="TIM" /> <xsd:enumeration value="TIMING_SYNCH" /> <xsd:enumeration value="TSD" /> <xsd:enumeration value="TSF" /> <xsd:enumeration value="TU-AIS" /> <xsd:enumeration value="TX_DEGRADE" /> <xsd:enumeration value="TX_FAIL" /> <xsd:enumeration value="TX_MIS_CONNECT" /> <xsd:enumeration value="TX_UNUSABLE_FE" /> <xsd:enumeration value="UAT" /> <xsd:enumeration value="UNEQ" /> <xsd:enumeration value="VC-AIS" /> <xsd:enumeration value="VC-RDI" /> <xsd:enumeration value="VP-AIS" /> <xsd:enumeration value="VP-RDI" /> <xsd:enumeration value="XPIC_FAIL" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI pre-defined specific TCM probable causes. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="TCM(_(AIS|LOS|OAI|RAI|SD|SSF|TIM|UNEQ|(LEVEL[1-6]_(LCK|LOS|OCI|RAI|SD|SSF|TIM))))?" /> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType> </xsd:element>

﻿

Uses
Type (1) string

Used-By

Generated by WSDLdoc ©