Operation void eventLossCleared (CIS GeneralizedTime endTime = NA), in Class NMSSession

Documentation
The EMS invokes this operation to indicate that the event or alarm loss period is over, and that it is now capable of providing relevant notifications.
After invoking this operation on the NmsSession instances, the EMS clears the internal flag set by alarmLossOccured() or/and eventLossOccurred. If event or alarm loss occurs again, alarmLossOccurred() or eventLossOccurred() will be called.
How and when the EMS decides to invoke eventLossCleared() is an EMS implementation detail. The actual algorithm that the EMS uses may be as simple as a timer-based mechanism or a complicated one which monitors the current rate at which the EMS pushes events.
Operation Exceptions:
None

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
The EMS has informed the NMS that an event has been discarded before.
Postconditions
The NMS is informed that EMS has resumed event forwarding.
Semantics

Arguments

endTime
/* in */ The time of the end of the event loss period, as determined by the EMS.