Class SNCCreateData {Analysis}

Documentation
Contains the read-create attributes that the NMS will pass to the EMS at SNC creation time.
Refer to the associated supporting document snctypes for explanation of SNC Properties, SNC Parameters, unidirectional SNCs, Point-to-Multipoint SNC, Routing Constraints and Route Discovery.
Object Lifecycle: This is part of SNC creation request. Lifecycle is limited to SNC lifecycle.
Object Creation Notification Issued? No
Object Deletion Notification Issued? No
External Documents

SD1-36_SNCTypes.pdf |

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
userLabel | SNCCreateData | CIS CharacterString | empty string
forceUniqueness | SNCCreateData | CIS Boolean | TRUE
owner | SNCCreateData | CIS CharacterString | empty string
networkAccessDomain | SNCCreateData | CIS CharacterString | empty string
direction | SNCCreateData | ConnectionDirection | BIDIRECTIONAL
staticProtectionLevel | SNCCreateData | StaticProtectionLevel | UNPROTECTED
protectionEffort | SNCCreateData | ProtectionEffort | WHATEVER
rerouteAllowed | SNCCreateData | RerouteAllowed | NO
networkRouted | SNCCreateData | NetworkRouted | NO
networkReroute | SNCCreateData | Reroute | Not_Set
sncType | SNCCreateData | SNCType | SIMPLE
layerRate | SNCCreateData | LayerRate | NA
fullRoute | SNCCreateData | CIS Boolean | FALSE
additionalCreationInfo | SNCCreateData | CIS SequenceOf Structs::AVP | empty list
bundledSNCIndicator | SNCCreateData | CIS Boolean | FALSE
mustRemoveGTPs | SNCCreateData | CIS Boolean | TRUE
priority | SNCCreateData | CIS Integer | 0
revertive | SNCCreateData | CIS Boolean | False
intendedRouteExclusive | SNCCreateData | CIS Boolean | True
alarmReportingIndication | SNCCreateData | CIS Boolean | FALSE
aEndPointsRole | SNCCreateData | CIS SequenceOf Structs::EndPointRole | NA
zEndPointsRole | SNCCreateData | CIS SequenceOf Structs::EndPointRole | NA
asapPointer | SNCCreateData | Name | CIS Null

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | --Not Named-- | SNCCreateData | ccInclusions | CrossConnect
--Not Named-- | --Not Named-- | SNCCreateData | tpInclusions | TerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | neInclusions | ManagedElement
--Not Named-- | --Not Named-- | SNCCreateData | sncExclusions | SubnetworkConnection
--Not Named-- | --Not Named-- | SNCCreateData | tpExclusions | TerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | neExclusions | ManagedElement
--Not Named-- | --Not Named-- | SNCCreateData | aEnd | ConnectionTerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | zEnd | ConnectionTerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | tlInclusions | TopologicalLink
--Not Named-- | --Not Named-- | SNCCreateData | tlExclusions | TopologicalLink
--Not Named-- | --Not Named-- | SNCCreateData | zEnd | GroupTerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | aEnd | GroupTerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | gtpInclusions | GroupTerminationPoint
--Not Named-- | --Not Named-- | SNCCreateData | gtpExclusions | GroupTerminationPoint