TPProtectionAssociation tpProtectionAssociation = NA, in Class TerminationPoint

Documentation
Indicates whether the TP has an associated protection TP and, if so, what kind of protection association exists.
Changes in the value of this attribute lead to a AVC notification.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? No

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No