tmf854.v1 > getAllTPPools_T LOCATION: file:/xsd/interfaces/MultiLayerSubnetworkMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The getAllTPPools_T Complex Type
This service returns all TP Pools within a Subnetwork contained in an OS. The TP Pool is a TP used to logically group TPs. The TP Pool does not affect TP containment. TP containment remains from the Network Element view. Given a TP Pool, the NMS could then determine all the TPs that are associated with the TP Pool, for the purpose of logical partitioning or grouping. See getTPGroupingRelationships(). Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if the OS does not support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when subnetworkName does not reference a multiLayerSubnetwork object EXCPT_ENTITY_NOT_FOUND - Raised when subnetworkName references an object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost

Local elements (1)
  subnetworkName

Complex Type getAllTPPools_T
The getAllTPPools_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> subnetworkName <subnetworkName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</subnetworkName> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="getAllTPPools_T"> -<xsd:annotation> <xsd:documentation> This service returns all TP Pools within a Subnetwork contained in an OS. The TP Pool is a TP used to logically group TPs. The TP Pool does not affect TP containment. TP containment remains from the Network Element view. Given a TP Pool, the NMS could then determine all the TPs that are associated with the TP Pool, for the purpose of logical partitioning or grouping. See getTPGroupingRelationships(). Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if the OS does not support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when subnetworkName does not reference a multiLayerSubnetwork object EXCPT_ENTITY_NOT_FOUND - Raised when subnetworkName references an object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="subnetworkName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> subnetworkName </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) getAllTPPools

Generated by WSDLdoc ©