Class TPPoolCreateData {Analysis}

Documentation
Contains the read-create attributes that the NMS will pass to the EMS at TPPool creation time.
Object Lifecycle: This is part of the TPPool creation request.
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
userLabel | TPPoolCreateData | CIS CharacterString | empty string
forceUniqueness | TPPoolCreateData | CIS Boolean | TRUE
owner | TPPoolCreateData | CIS CharacterString | empty string
containedMembers | TPPoolCreateData | CIS SequenceOf Name | NA
descriptionOfUse | TPPoolCreateData | CIS CharacterString | empty string
additionalCreationInfo | TPPoolCreateData | CIS SequenceOf Structs::AVP | empty list

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | --Not Named-- | TPPoolCreateData | commonTransmissionParameters | CommonTransmissionParameters