Operation void getTCAParameter (Name pmp = NA, PMParameterName pmParameter = NA, CIS SequenceOf PMThreshold pmThresholds = NA), in Class TerminationPoint

Documentation
This operation is used to query all currently applied TCA parameters on a PM Parameter within a PMP.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when any input parameter is syntactically incorrect.
3. ENTITY_NOT_FOUND - Raised when PMP does not exist.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

pmp
/* in */ The PMP for which the thresholds of specified PM Parameter has to be returned.
pmParameter
/* in */ PM Parameter for which the PM Thresholds have to be returned.
pmThresholds
/* out */ List of TCA thresholds.