Class EMS {Analysis} derived from: CommonResourceInfo

Documentation
The EMS represents the Element Management System (EMS), and its management domain.
Object Lifecycle: Created and Deleted only by the EMS
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Operations

Name | Signature | Class
getAllEMSSystemActiveAlarms | void getAllEMSSystemActiveAlarms (CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList = empty list, CIS SequenceOf AlarmInformation activeAlarmList = empty list) | EMS
getAllTopLevelSubnetworks | void getAllTopLevelSubnetworks (CIS SequenceOf Subnetwork subnetworkList) | EMS
getAllTopLevelSubnetworkNames | void getAllTopLevelSubnetworkNames (CIS SequenceOf Name nameList = empty list) | EMS
getMultiLayerSubnetwork | void getMultiLayerSubnetwork (Name subnetName, MultiLayerSubnetwork subnetwork) | EMS
getAllTopLevelTopologicalLinks | void getAllTopLevelTopologicalLinks (CIS SequenceOf TopologicalLink topologicalLinkList = empty list) | EMS
getAllTopLevelTopologicalLinkNames | void getAllTopLevelTopologicalLinkNames (CIS SequenceOf Name nameList = empty list) | EMS
getTopLevelTopologicalLink | void getTopLevelTopologicalLink (Name topoLinkName, TopologicalLink topoLink) | EMS
getAllEMSAndMEActiveAlarms | void getAllEMSAndMEActiveAlarms (CIS SequenceOf Strings::ProbableCause excludeProbCauseList = empty list, CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList = empty list, CIS SequenceOf AlarmInformation activeAlarmList = empty list) | EMS
getAllManagedElements | void getAllManagedElements (CIS SequenceOf ManagedElement meList = empty list) | EMS
getAllManagedElementNames | void getAllManagedElementNames (CIS SequenceOf Name meNameList = empty list) | EMS
getManagedElement | void getManagedElement (Name meName = NA, ManagedElement me = NA) | EMS
getGCTProfileInfo | void getGCTProfileInfo (GCTProfileInfo gctProfileInfo = NA) | EMS
launchGCT | void launchGCT (Name objectName = NA, CIS CharacterString context = NA, CIS SequenceOf Structs::AVP userInfo = NA, CIS CharacterString gctDisplayAddress = NA, CIS SequenceOf Structs::AVP additionalInfoInputList = empty list, CIS Boolean. closingEnabled, CIS SequenceOf Structs::AVP additionalInfoOutputList) | EMS
destroyGCT | void destroyGCT ( CIS CharacterString gCTDisplayAddress = NA) | EMS
getAllTrafficDescriptors | void getAllTrafficDescriptors (CIS SequenceOf TrafficDescriptor trafficDescriptors = empty list) | EMS
getAllTrafficDescriptorNames | void getAllTrafficDescriptorNames (CIS SequenceOf Name trafficDescriptorNames = empty list) | EMS
getTrafficDescriptor | void getTrafficDescriptor (Name tdName = NA, TrafficDescriptor trafficDescriptor = NA) | EMS
createTrafficDescriptor | void createTrafficDescriptor (TDCreateData newTDcreateData, TrafficDescriptor newTD) | EMS
deleteTrafficDescriptor | void deleteTrafficDescriptor (Name trafficDescriptorName) | EMS
getCapabilities | void getCapabilities (CIS SequenceOf Structs::AVP capabilities) | EMS
createTopologicalLink | void createTopologicalLink (TLCreateData tlCreateData, TopologicalLink topologicalLink) | EMS
deleteTopologicalLink | void deleteTopologicalLink (Name topologicalLinkName) | EMS
acknowledgeAlarms | void acknowledgeAlarms (CIS SequenceOf of Choice alarmOrTCAIdList, CIS SequenceOf Structs::AVP additionalInfo = empty list, CIS SequenceOf of Choice failedAlarmOrTCAIdList = empty list) | EMS
unacknowledgeAlarms | void unacknowledgeAlarms (CIS SequenceOf of Choice alarmOrTCAIdList, CIS SequenceOf Structs::AVP additionalInfo = empty list, CIS SequenceOf of Choice failedAlarmOrTCAIdList = empty list) | EMS
getAllEMSAndMEUnacknowledgedActiveAlarms | void getAllEMSAndMEUnacknowledgedActiveAlarms (CIS SequenceOf Strings::ProbableCause excludeProbCauseList = empty list, CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList = empty list, CIS SequenceOf Choice alarmTCAList = empty list) | EMS
getAllEMSSystemUnacknowledgedActiveAlarms | void getAllEMSSystemUnacknowledgedActiveAlarms (CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList = empty list, CIS SequenceOf Choice alarmTCAList = empty list) | EMS
getAllTransmissionDescriptors | void getAllTransmissionDescriptors (CIS SequenceOf TransmissionDescriptor transmissionDescriptors) | EMS
getAllTransmissionDescriptorNames | void getAllTransmissionDescriptorNames (CIS SequenceOf Name transmissionDescriptorNames ) | EMS
getTransmissionDescriptor | void getTransmissionDescriptor (Name transmissionDescriptorName = NA, TransmissionDescriptor transmissionDescriptor = NA) | EMS
createTransmissionDescriptor | void createTransmissionDescriptor (TransmissionDescriptorCreateData transmissionDescriptorCreateData = NA, TransmissionDescriptor newTD = NA) | EMS
deleteTransmissionDescriptor | void deleteTransmissionDescriptor (Name trafficDescriptorName) | EMS
getLog | void getLog (Log logInformation = NA) | EMS
createASAP | void createASAP (ASAPCreateModifyData newASAPCreateData = NA, AlarmSeverityAssignmentProfile newASAP = NA) | EMS
deleteASAP | void deleteASAP (Name asapName = NA, CIS SequenceOf Structs::AVP additionalInfo = empty list) | EMS
assignASAP | void assignASAP (Name asapName = NA, Name resourceName = NA, LayerRate layerRate = LR_Not_Applicable, CIS SequenceOf Structs::AVP additionalInfo = empty list) | EMS
deassignASAP | void deassignASAP (Name resourceName = CIS Null, LayerRate layerRate = LR_Not_Applicable, CIS SequenceOf Structs::AVP additionalInfo = empty list) | EMS
modifyASAP | void modifyASAP (Name asapName = NA, ASAPCreateModifyData asapModifyData = NA, AlarmSeverityAssignmentProfile newASAP = NA) | EMS
getAllASAPs | void getAllASAPs (CIS SequenceOf AlarmSeverityAssignmentProfile asapList = empty list) | EMS
getAllASAPNames | void getAllASAPNames (CIS SequenceOf Name asapNameList = empty list) | EMS
getASAP | void getASAP (Name asapName = NA, AlarmSeverityAssignmentProfile asap = empty list) | EMS
getASAPByResource | void getASAPByResource (Name resourceName = NA, CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf AlarmSeverityAssignmentProfile asapList = empty list) | EMS
getEMS | void getEMS (EMS ems) | EMS
setNativeEMSName | void setNativeEMSName (Name objectName, CIS CharcaterString nativeEMSName) | CommonResourceInfo
setOwner | void setOwner (Name objectName, CIS CharcaterString owner) | CommonResourceInfo
setUserLabel | void setUserLabel (Name objectName, CIS CharcaterString userLabel, Boolean enforceUniqueness) | CommonResourceInfo
setNetworkAccessDomain | void setNetworkAccessDomain (CIS CharcaterString networkAccessDomain = NA) | CommonResourceInfo
setAdditionalInfo | void setAdditionalInfo (CIS SequenceOf Structs::AVP additionalInfo = empty list) | CommonResourceInfo

Attributes

Name | Class | Type | Initial Value
emsVersion | EMS | CIS CharacterString | empty string
type | EMS | CIS CharacterString | empty string
asapPointer | EMS | Name | CIS Null
name | CommonResourceInfo | Name | NA
userLabel | CommonResourceInfo | CIS CharacterString | Value of the nativeEMSName attribute.
owner | CommonResourceInfo | CIS CharacterString | empty string
nativeEMSName | CommonResourceInfo | CIS CharacterString | empty string
discoveredName | CommonResourceInfo | CIS CharacterString | empty string
namingOS | CommonResourceInfo | Name | CIS Null
source | CommonResourceInfo | ObjectSource | UNKNOWN
aliasNameList | CommonResourceInfo | AVP | empty list
resourceState | CommonResourceInfo | ResourceState | UNKNOWN
additionalInfo | CommonResourceInfo | CIS SequenceOf Structs::AVP | empty list

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | --Not Named-- | EMS | --Not Named-- | MultiLayerSubnetwork
--Not Named-- | --Not Named-- | EMS | --Not Named-- | TopologicalLink
--Not Named-- | --Not Named-- | EMS | --Not Named-- | TrafficDescriptor
retrieve active | --Not Named-- | EMS | --Not Named-- | AlarmInformation
--Not Named-- | --Not Named-- | EMS | --Not Named-- | ManagedElement
--Not Named-- | --Not Named-- | EMS | --Not Named-- | PerformanceManager
--Not Named-- | --Not Named-- | EMS | --Not Named-- | Log
--Not Named-- | --Not Named-- | EMS | --Not Named-- | SoftwareManager
--Not Named-- | --Not Named-- | EMS | --Not Named-- | TransmissionDescriptor
--Not Named-- | --Not Named-- | EMS | --Not Named-- | AlarmSeverityAssignmentProfile
--Not Named-- | --Not Named-- | EMS | --Not Named-- | AlarmSeverityAssignmentProfile

Dependencies

Name | Class | Supplier
generates | EMS | AlarmInformation
reports | EMS | ObjectInformation
cut-through | EMS | GCTProfileInfo
create TL with | EMS | TLCreateData
create TD with | EMS | TDCreateData
createTMD with | EMS | TransmissionDescriptorCreateData
create ASAP with | EMS | ASAPCreateModifyData

Generalization Relationships

Name | Class | Supplier
--Not Named-- | EMS | CommonResourceInfo

Realize Relationships

Name | Class | Supplier
--Not Named-- | EMS | Supplier
--Not Named-- | EMS | SessionFactory
--Not Named-- | EMS | Consumer