tmf854.v1 > TPConnectionState_T LOCATION: file:/xsd/networkResources/TerminationPoint.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The TPConnectionState_T Simple Type
A CTP/FTP may be involved in zero, one, or many connections. The value TPConnectionState indicates the degree to which a CTP/FTP is used. The values TPCS_SOURCE_CONNECTED and TPCS_SINK_CONNECTED reflect the presence of a one way connection. The value TPCS_BI_CONNECTED means that the TP is both sink and source connected. If an EMS cannot report whether the source of the TP is connected or the sink is connected, TPCS_BI_CONNECTED may be reported by that EMS. The value TPCS_NA is used for PTPs and TPPools.
Simple Type TPConnectionState_T
TPConnectionState_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (TPCS_NA | TPCS_SOURCE_CONNECTED | TPCS_SINK_CONNECTED | TPCS_BI_CONNECTED | TPCS_NOT_CONNECTED).

Enumeration | Description
TPCS_NA |
TPCS_SOURCE_CONNECTED |
TPCS_SINK_CONNECTED |
TPCS_BI_CONNECTED |
TPCS_NOT_CONNECTED |

XML
-<xsd:simpleType name="TPConnectionState_T"> -<xsd:annotation> <xsd:documentation> A CTP/FTP may be involved in zero, one, or many connections. The value TPConnectionState indicates the degree to which a CTP/FTP is used. The values TPCS_SOURCE_CONNECTED and TPCS_SINK_CONNECTED reflect the presence of a one way connection. The value TPCS_BI_CONNECTED means that the TP is both sink and source connected. If an EMS cannot report whether the source of the TP is connected or the sink is connected, TPCS_BI_CONNECTED may be reported by that EMS. The value TPCS_NA is used for PTPs and TPPools. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="TPCS_NA" /> <xsd:enumeration value="TPCS_SOURCE_CONNECTED" /> <xsd:enumeration value="TPCS_SINK_CONNECTED" /> <xsd:enumeration value="TPCS_BI_CONNECTED" /> <xsd:enumeration value="TPCS_NOT_CONNECTED" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (2) ConnectionTerminationPoint_T/connectionState FloatingTerminationPoint_T/connectionState

Generated by WSDLdoc ©