tmf854.v1 > getAssociatedTP_T LOCATION: file:/xsd/interfaces/MultiLayerSubnetworkMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The getAssociatedTP_T Complex Type
This service returns a list of PSR (UPSR or SNCP) associated termination points for the TP whose name is passed as a parameter. Note: The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. When this service is invoked with a TP that is not an edge point, the returned TPs will be on the same Managed Element Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if OS cannot support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a CTP, FTP or PTP. EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a CTP, FTP or PTP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost

Local elements (1)
  tpName

Complex Type getAssociatedTP_T
The getAssociatedTP_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> The name of the TP for which to retrieve associated TPs <tpName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</tpName> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="getAssociatedTP_T"> -<xsd:annotation> <xsd:documentation> This service returns a list of PSR (UPSR or SNCP) associated termination points for the TP whose name is passed as a parameter. Note: The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. When this service is invoked with a TP that is not an edge point, the returned TPs will be on the same Managed Element Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if OS cannot support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a CTP, FTP or PTP. EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a CTP, FTP or PTP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="tpName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> The name of the TP for which to retrieve associated TPs </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) getAssociatedTP

Generated by WSDLdoc ©