tmf854.v1 > getContainingTPs_T LOCATION: file:/xsd/interfaces/ManagedElementMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The getContainingTPs_T Complex Type
This service returns a list of the containing TPs given a CTP. This will return an PTP or FTP where there is only one level of containment. In a case of deeper containment this will return a list of CTPs and a PTP or FTP. Using the UPSR OC3 example used in getContainedPotentialTPs, getContainingTPs on the working T1 CTP will return a working STS1 CTP and a working OC3PTP. If the OC3 was in APS, then getContainingTPs on the T1 CTP would return an STS1 CTP, an OC3 working PTP and an OC3 protect PTP. Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if OS cannot support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a CTP object EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a CTP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost

Local elements (1)
  tpName

Complex Type getContainingTPs_T
The getContainingTPs_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> Name of the CTP for which containing CTPs and PTP/FTP are to be reported. The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. <tpName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</tpName> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="getContainingTPs_T"> -<xsd:annotation> <xsd:documentation> This service returns a list of the containing TPs given a CTP. This will return an PTP or FTP where there is only one level of containment. In a case of deeper containment this will return a list of CTPs and a PTP or FTP. Using the UPSR OC3 example used in getContainedPotentialTPs, getContainingTPs on the working T1 CTP will return a working STS1 CTP and a working OC3PTP. If the OC3 was in APS, then getContainingTPs on the T1 CTP would return an STS1 CTP, an OC3 working PTP and an OC3 protect PTP. Refer to the TMF 854 XML Solution Set document for details on the Message Exchange Pattern controls (multiple batch response). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if OS cannot support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a CTP object EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a CTP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="tpName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> Name of the CTP for which containing CTPs and PTP/FTP are to be reported. The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) getContainingTPs

Generated by WSDLdoc ©