This object represents the information in a log AVC notification.
The AVC event is generated by a log when one of the following log attributes have changed:
- capacity alarm threshold
- log full action
- maximum log size
- start time
- stop time
- week mask
- changing the discrimnator constraint
- max record life

Object Lifecycle: Created and deleted by EMS.

Object Creation Notification Issued? No
Object Deletion Notification Issued? No
