CIS Boolean rootCauseAlarmIndication = NA, in Class AlarmInformation

Documentation
This attribute indicates whether an alarm is a raw (uncorrelated) alarm or a root cause alarm indication.
The attribute can have two values:
- TRUE (meaning that the alarm is a Root Cause Alarm Indication)
- FALSE (meaning the alarm is a raw alarm).
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No