Operation void getAllActiveAlarms (CIS SequenceOf Strings::ProbableCause excludeProbCauseList, CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList, CIS SequenceOf AlarmInformation activeAlarms), in Class ManagedElement

Documentation
Get all active alarms and TCAs.
Note: A raised alarm is called active as long as no clear notification was received.
Alarms that are not reported by the ME to the EMS should not be reported by this operation.
Alarms which ASAP assigned severity is "NOT_ALARMED" should not be reported by this operation.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when excludeProbCauseList or excludeSeverityList contains undefined values.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

excludeProbCauseList
/* in */ The list of probable causes to exclude (for which events should not be reported).
excludeSeverityList
/* in */ List of severities to exclude from the output event list.
activeAlarms
/* out */ The list of active alarms.