Operation void deleteTCAParameterProfile (Name tcaParameterProfileName = NA), in Class PerformanceManager

Documentation
Deletes a TCA Parameter Profile.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when specified TCA Parameter Profile does not exist.
5. OBJECT_IN_USE - Raised when TCA Parameter Profile is still assigned to at least one TP.
6. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
1. The profile to be deleted has to exist.
2. The profile to be deleted must not be assigned to any TP.
Postconditions
TCA Parameter Profile no longer exist.
Semantics

Arguments

tcaParameterProfileName
/* in */ The EMS defined name of the profile to be deleted.