tmf854.v1 > Hitless_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The Hitless_T Simple Type
This attribute specifies whether the hitless switching capability (i.e. a switch event between a working and a protection channel which does not add any errors to those already produced by the propagation medium during the switching procedure) is present or not. A value of "Yes" indicates that the hitless capability is present in the protection system. A value of "No" indicates that the hitless capability is not present and will as a consequence introduce errors on a switch operation. See G.774.08.
<ApplicableTo>1+1 trail protection,1:N trail protection</ApplicableTo>
Simple Type Hitless_T
Hitless_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (Yes | No).

Enumeration | Description
Yes |
No |

XML
-<xsd:simpleType name="Hitless_T"> -<xsd:annotation> -<xsd:documentation> This attribute specifies whether the hitless switching capability (i.e. a switch event between a working and a protection channel which does not add any errors to those already produced by the propagation medium during the switching procedure) is present or not. A value of "Yes" indicates that the hitless capability is present in the protection system. A value of "No" indicates that the hitless capability is not present and will as a consequence introduce errors on a switch operation. See G.774.08. <ApplicableTo>1+1 trail protection,1:N trail protection</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="Yes" /> <xsd:enumeration value="No" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/Hitless

Generated by WSDLdoc ©