Operation void getSNCsByUserLabel (CIS CharacterString userLabel = NA, CIS SequenceOf SubnetworkConnection sncList = NA), in Class MultiLayerSubnetwork

Documentation
This operation will return the SubnetworkConnections whose userLabel is supplied as a parameter.
This operation also works for bundled SNCs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

userLabel
/* in */ The user label of the SNCs to retrieve.
sncList
/* out */ The SNCs matching the user label.