Class ProtectionGroupType {Analysis}

Documentation
Note: The values "MSP_1_PLUS_1" and "MSP_1_FOR_N" are also used for trail protection.
Object Lifecycle: NA
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Enums | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
MSP_1_PLUS_1 | ProtectionGroupType | Integer | 0
MSP_1_FOR_N | ProtectionGroupType | Integer | 1
2_FIBER_BLSR | ProtectionGroupType | Integer | 2
4_FIBER_BLSR | ProtectionGroupType | Integer | 3