Reroute networkReroute = Not_Set, in Class SNCCreateData

Documentation
Indicates if the reroute (if allowed) should be computed by the network (Yes), by the EMS (No), or if it does not matter (Not_Set).
Changes in the value of this attribute shall lead to an AVC notification.
Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No