tmf854.v1 > LayerRate_T LOCATION: file:/xsd/networkResources/LayerRates.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The LayerRate_T Simple Type
The LayerRate_T value is used to identify: - the Layer of a PTP/CTP, - the characteristic information of a PTP/FTP, - the Layer/Rate of a connection. Each LayerRate_T may be used in conjunction with a CTP/PTP/FTP of that layer. In the SDH definitions, the G.805 CP and G.805 Termination Function layer names differ, for example TU12 is used for the G.805 CP and VC12 for the corresponding G.805 Termination Function. In this interface definition the TU and VC definitions have been combined into a single composite layer and this has been named to include the equivalent SONET layer, e.g. LR_VT2_and_TU12_VC12. For more details refer to the following supporting document: - layering documentfor all layering concepts - LayerRates document for information about recognized values in MTOSI Any vendor extensions are permitted. However, they shall comply with MTOSI attribute vendor extension rule: Values must have the "PROP_" prefix. Refer to the TMF 854 XML Solution Set document for more details.
Simple Type LayerRate_T
LayerRate_T is union of (string, string, string).
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`PROP_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (LR_DS0_64K | LR_DSL | LR_Not_Applicable | LR_Async_FOTS_150M | LR_Async_FOTS_417M | LR_Async_FOTS_560M | LR_Async_FOTS_565M | LR_Async_FOTS_1130M | LR_Async_FOTS_1G7 | LR_Async_FOTS_1G8 | LR_ATM_NI | LR_ATM_VC | LR_ATM_VP | LR_D1_Video | LR_DIGITAL_SIGNAL_RATE | LR_DIGITAL_SIGNAL_RATE | LR_PHYSICAL_ELECTRICAL. | LR_DSR_1_5M | LR_DSR_2M | LR_DSR_4M | LR_DSR_6M | LR_DSR_8M | LR_DSR_16M | LR_DSR_34M | LR_E2_8M | LR_E5_565M | LR_Encapsulation | LR_Fragment | LR_DSR_45M | LR_DSR_140M | LR_DSR_565M | LR_DSR_Fast_Ethernet | LR_DSR_Gigabit_Ethernet | LR_DSR_10Gigabit_Ethernet | LR_DSR_OC1_STM0 | LR_DSR_OC3_STM1 | LR_DSR_2xSTM1 | LR_DSR_OC12_STM4 | LR_DSR_OC24_STM8 | LR_DSR_OC48_and_STM16 | LR_DSR_OC192_and_STM64 | LR_DSR_OC768_and_STM256 | LR_DSR_OTU1 | LR_DSR_OTU2 | LR_DSR_OTU3 | LR_E1_2M | LR_E20_2x2M | LR_E30_8x2M | LR_E3_34M | LR_E4_140M | LR_ESCON | LR_Ethernet | LR_ETR | LR_Fast_Ethernet | LR_FC_12_133M | LR_FC_25_266M | LR_FC_50_531M | LR_FC_100_1063M | LR_FDDI | LR_FICON | LR_FR_IF | LR_FR_PVC | LR_Gigabit_Ethernet | LR_ISDN_BRI | LR_Line_OC1_STS1_and_MS_STM0 | LR_Line_OC3_STS3_and_MS_STM1 | LR_Line_OC12_STS12_and_MS_STM4 | LR_Line_OC24_STS24_and_MS_STM8 | LR_Line_OC48_STS48_and_MS_STM16 | LR_Line_OC192_STS192_and_MS_STM64 | LR_Line_OC768_STS768_and_MS_STM256 | LR_Low_Order_TU3_VC3 | LR_OCH_Data_Unit_1 | LR_OCH_Data_Unit_2 | LR_OCH_Data_Unit_3 | LR_OCH_Transport_Unit_1 | LR_OCH_Transport_Unit_2 | LR_OCH_Transport_Unit_3 | LR_STS3c_and_AU4_VC4 | LR_STS4c_and_VC3_4c | LR_STS5c_and_VC3_5c | LR_STS6c_and_VC4_2c | LR_STS7c_and_VC3_7c | LR_STS8c_and_VC3_8c | LR_STS9c_and_VC4_3c | LR_Optical_Channel | LR_Optical_Multiplex_Section | LR_OPTICAL_SECTION | LR_Optical_Transmission_Section | LR_PHYSICAL_ELECTRICAL | LR_PHYSICAL_MEDIALESS | LR_PHYSICAL_OPTICAL | LR_POTS | LR_Section_OC1_STS1_and_RS_STM0 | LR_Section_OC3_STS3_and_RS_STM1 | LR_Section_OC12_STS12_and_RS_STM4 | LR_Section_OC24_STS24_and_RS_STM8 | LR_Section_OC48_STS48_and_RS_STM16 | LR_Section_OC192_STS192_and_RS_STM64 | LR_Section_OC768_STS768_and_RS_STM256 | LR_STS1_and_AU3_High_Order_VC3 | LR_STS2c_and_VC3_2c | LR_STS10c_and_VC3_10c | LR_STS11c_and_VC3_11c | LR_STS12c_and_VC4_4c | LR_STS13c_and_VC3_13c | LR_STS14c_and_VC3_14c | LR_STS15c_and_VC4_5c | LR_STS16c_and_VC3_16c | LR_STS17c_and_VC3_17c | LR_STS18c_and_VC4_6c | LR_STS19c_and_VC3_19c | LR_STS20c_and_VC3_20c | LR_STS21c_and_VC4_7c | LR_STS22c_and_VC3_22c | LR_STS23c_and_VC3_23c | LR_STS24c_and_VC4_8c | LR_STS25c_and_VC3_25c | LR_STS26c_and_VC3_26c | LR_STS27c_and_VC4_9c | LR_STS28c_and_VC3_28c | LR_STS29c_and_VC3_29c | LR_STS30c_and_VC4_10c | LR_STS31c_and_VC3_31c | LR_STS32c_and_VC3_32c | LR_STS33c_and_VC4_11c | LR_STS34c_and_VC3_34c | LR_STS35c_and_VC3_35c | LR_STS36c_and_VC4_12c | LR_STS37c_and_VC3_37c | LR_STS38c_and_VC3_38c | LR_STS39c_and_VC4_13c | LR_STS40c_and_VC3_40c | LR_STS41c_and_VC3_41c | LR_STS42c_and_VC4_14c | LR_STS43c_and_VC3_43c | LR_STS44c_and_VC3_44c | LR_STS45c_and_VC4_15c | LR_STS46c_and_VC3_46c | LR_STS47c_and_VC3_47c | LR_STS48c_and_VC4_16c | LR_STS49c_and_VC3_49c | LR_STS50c_and_VC3_50c | LR_STS51c_and_VC4_17c | LR_STS52c_and_VC3_52c | LR_STS53c_and_VC3_53c | LR_STS54c_and_VC4_18c | LR_STS55c_and_VC3_55c | LR_STS56c_and_VC3_56c | LR_STS57c_and_VC4_19c | LR_STS58c_and_VC3_58c | LR_STS59c_and_VC3_59c | LR_STS60c_and_VC4_20c | LR_STS61c_and_VC3_61c | LR_STS62c_and_VC3_62c | LR_STS63c_and_VC4_21c | LR_STS64c_and_VC3_64c | LR_STS65c_and_VC3_65c | LR_STS66c_and_VC4_22c | LR_STS67c_and_VC3_67c | LR_STS68c_and_VC3_68c | LR_STS69c_and_VC4_23c | LR_STS70c_and_VC3_70c | LR_STS71c_and_VC3_71c | LR_STS72c_and_VC4_24c | LR_STS73c_and_VC3_73c | LR_STS74c_and_VC3_74c | LR_STS75c_and_VC4_25c | LR_STS76c_and_VC3_76c | LR_STS77c_and_VC3_77c | LR_STS78c_and_VC4_26c | LR_STS79c_and_VC3_79c | LR_STS80c_and_VC3_80c | LR_STS81c_and_VC4_27c | LR_STS82c_and_VC3_82c | LR_STS83c_and_VC3_83c | LR_STS84c_and_VC4_28c | LR_STS85c_and_VC3_85c | LR_STS86c_and_VC3_86c | LR_STS87c_and_VC4_29c | LR_STS88c_and_VC3_88c | LR_STS89c_and_VC3_89c | LR_STS90c_and_VC4_30c | LR_STS91c_and_VC3_91c | LR_STS92c_and_VC3_92c | LR_STS93c_and_VC4_31c | LR_STS94c_and_VC3_94c | LR_STS95c_and_VC3_95c | LR_STS96c_and_VC4_32c | LR_STS97c_and_VC3_97c | LR_STS98c_and_VC3_98c | LR_STS99c_and_VC4_33c | LR_STS100c_and_VC3_100c | LR_STS101c_and_VC3_101c | LR_STS102c_and_VC4_34c | LR_STS103c_and_VC3_103c | LR_STS104c_and_VC3_104c | LR_STS105c_and_VC4_35c | LR_STS106c_and_VC3_106c | LR_STS107c_and_VC3_107c | LR_STS108c_and_VC4_36c | LR_STS109c_and_VC3_109c | LR_STS110c_and_VC3_110c | LR_STS111c_and_VC4_37c | LR_STS112c_and_VC3_112c | LR_STS113c_and_VC3_113c | LR_STS114c_and_VC4_38c | LR_STS115c_and_VC3_115c | LR_STS116c_and_VC3_116c | LR_STS117c_and_VC4_39c | LR_STS118c_and_VC3_118c | LR_STS119c_and_VC3_119c | LR_STS120c_and_VC4_40c | LR_STS121c_and_VC3_121c | LR_STS122c_and_VC3_122c | LR_STS123c_and_VC4_41c | LR_STS124c_and_VC3_124c | LR_STS125c_and_VC3_125c | LR_STS126c_and_VC4_42c | LR_STS127c_and_VC3_127c | LR_STS128c_and_VC3_128c | LR_STS129c_and_VC4_43c | LR_STS130c_and_VC3_130c | LR_STS131c_and_VC3_131c | LR_STS132c_and_VC4_44c | LR_STS133c_and_VC3_133c | LR_STS134c_and_VC3_134c | LR_STS135c_and_VC4_45c | LR_STS136c_and_VC3_136c | LR_STS137c_and_VC3_137c | LR_STS138c_and_VC4_46c | LR_STS139c_and_VC3_139c | LR_STS140c_and_VC3_140c | LR_STS141c_and_VC4_47c | LR_STS142c_and_VC3_142c | LR_STS143c_and_VC3_143c | LR_STS144c_and_VC4_48c | LR_STS145c_and_VC3_145c | LR_STS146c_and_VC3_146c | LR_STS147c_and_VC4_49c | LR_STS148c_and_VC3_148c | LR_STS149c_and_VC3_149c | LR_STS150c_and_VC4_50c | LR_STS151c_and_VC3_151c | LR_STS152c_and_VC3_152c | LR_STS153c_and_VC4_51c | LR_STS154c_and_VC3_154c | LR_STS155c_and_VC3_155c | LR_STS156c_and_VC4_52c | LR_STS157c_and_VC3_157c | LR_STS158c_and_VC3_158c | LR_STS159c_and_VC4_53c | LR_STS160c_and_VC3_160c | LR_STS161c_and_VC3_161c | LR_STS162c_and_VC4_54c | LR_STS163c_and_VC3_163c | LR_STS164c_and_VC3_164c | LR_STS165c_and_VC4_55c | LR_STS166c_and_VC3_166c | LR_STS167c_and_VC3_167c | LR_STS168c_and_VC4_56c | LR_STS169c_and_VC3_169c | LR_STS170c_and_VC3_170c | LR_STS171c_and_VC4_57c | LR_STS172c_and_VC3_172c | LR_STS173c_and_VC3_173c | LR_STS174c_and_VC4_58c | LR_STS175c_and_VC3_175c | LR_STS176c_and_VC3_176c | LR_STS177c_and_VC4_59c | LR_STS178c_and_VC3_178c | LR_STS179c_and_VC3_179c | LR_STS180c_and_VC4_60c | LR_STS181c_and_VC3_181c | LR_STS182c_and_VC3_182c | LR_STS183c_and_VC4_61c | LR_STS184c_and_VC3_184c | LR_STS185c_and_VC3_185c | LR_STS186c_and_VC4_62c | LR_STS187c_and_VC3_187c | LR_STS188c_and_VC3_188c | LR_STS189c_and_VC4_63c | LR_STS190c_and_VC3_190c | LR_STS191c_and_VC3_191c | LR_STS192c_and_VC4_64c | LR_STS768c_and_VC4_256c | LR_T1_and_DS1_1_5M | LR_T2_and_DS2_6M | LR_T3_and_DS3_45M | LR_VT1_5_and_TU11_VC11 | LR_VT2_and_TU12_VC12 | LR_VT6_and_TU2_VC2).

Enumeration | Description
LR_DS0_64K |
LR_DSL |
LR_Not_Applicable |
LR_Async_FOTS_150M |
LR_Async_FOTS_417M |
LR_Async_FOTS_560M |
LR_Async_FOTS_565M |
LR_Async_FOTS_1130M |
LR_Async_FOTS_1G7 |
LR_Async_FOTS_1G8 |
LR_ATM_NI |
LR_ATM_VC |
LR_ATM_VP |
LR_D1_Video |
LR_DIGITAL_SIGNAL_RATE |
LR_DIGITAL_SIGNAL_RATE |
LR_PHYSICAL_ELECTRICAL. |
LR_DSR_1_5M |
LR_DSR_2M |
LR_DSR_4M |
LR_DSR_6M |
LR_DSR_8M |
LR_DSR_16M |
LR_DSR_34M |
LR_E2_8M |
LR_E5_565M |
LR_Encapsulation |
LR_Fragment |
LR_DSR_45M |
LR_DSR_140M |
LR_DSR_565M |
LR_DSR_Fast_Ethernet |
LR_DSR_Gigabit_Ethernet |
LR_DSR_10Gigabit_Ethernet |
LR_DSR_OC1_STM0 |
LR_DSR_OC3_STM1 |
LR_DSR_2xSTM1 |
LR_DSR_OC12_STM4 |
LR_DSR_OC24_STM8 |
LR_DSR_OC48_and_STM16 |
LR_DSR_OC192_and_STM64 |
LR_DSR_OC768_and_STM256 |
LR_DSR_OTU1 |
LR_DSR_OTU2 |
LR_DSR_OTU3 |
LR_E1_2M |
LR_E20_2x2M |
LR_E30_8x2M |
LR_E3_34M |
LR_E4_140M |
LR_ESCON |
LR_Ethernet |
LR_ETR |
LR_Fast_Ethernet |
LR_FC_12_133M |
LR_FC_25_266M |
LR_FC_50_531M |
LR_FC_100_1063M |
LR_FDDI |
LR_FICON |
LR_FR_IF |
LR_FR_PVC |
LR_Gigabit_Ethernet |
LR_ISDN_BRI |
LR_Line_OC1_STS1_and_MS_STM0 |
LR_Line_OC3_STS3_and_MS_STM1 |
LR_Line_OC12_STS12_and_MS_STM4 |
LR_Line_OC24_STS24_and_MS_STM8 |
LR_Line_OC48_STS48_and_MS_STM16 |
LR_Line_OC192_STS192_and_MS_STM64 |
LR_Line_OC768_STS768_and_MS_STM256 |
LR_Low_Order_TU3_VC3 |
LR_OCH_Data_Unit_1 |
LR_OCH_Data_Unit_2 |
LR_OCH_Data_Unit_3 |
LR_OCH_Transport_Unit_1 |
LR_OCH_Transport_Unit_2 |
LR_OCH_Transport_Unit_3 |
LR_STS3c_and_AU4_VC4 |
LR_STS4c_and_VC3_4c |
LR_STS5c_and_VC3_5c |
LR_STS6c_and_VC4_2c |
LR_STS7c_and_VC3_7c |
LR_STS8c_and_VC3_8c |
LR_STS9c_and_VC4_3c |
LR_Optical_Channel |
LR_Optical_Multiplex_Section |
LR_OPTICAL_SECTION |
LR_Optical_Transmission_Section |
LR_PHYSICAL_ELECTRICAL |
LR_PHYSICAL_MEDIALESS |
LR_PHYSICAL_OPTICAL |
LR_POTS |
LR_Section_OC1_STS1_and_RS_STM0 |
LR_Section_OC3_STS3_and_RS_STM1 |
LR_Section_OC12_STS12_and_RS_STM4 |
LR_Section_OC24_STS24_and_RS_STM8 |
LR_Section_OC48_STS48_and_RS_STM16 |
LR_Section_OC192_STS192_and_RS_STM64 |
LR_Section_OC768_STS768_and_RS_STM256 |
LR_STS1_and_AU3_High_Order_VC3 |
LR_STS2c_and_VC3_2c |
LR_STS10c_and_VC3_10c |
LR_STS11c_and_VC3_11c |
LR_STS12c_and_VC4_4c |
LR_STS13c_and_VC3_13c |
LR_STS14c_and_VC3_14c |
LR_STS15c_and_VC4_5c |
LR_STS16c_and_VC3_16c |
LR_STS17c_and_VC3_17c |
LR_STS18c_and_VC4_6c |
LR_STS19c_and_VC3_19c |
LR_STS20c_and_VC3_20c |
LR_STS21c_and_VC4_7c |
LR_STS22c_and_VC3_22c |
LR_STS23c_and_VC3_23c |
LR_STS24c_and_VC4_8c |
LR_STS25c_and_VC3_25c |
LR_STS26c_and_VC3_26c |
LR_STS27c_and_VC4_9c |
LR_STS28c_and_VC3_28c |
LR_STS29c_and_VC3_29c |
LR_STS30c_and_VC4_10c |
LR_STS31c_and_VC3_31c |
LR_STS32c_and_VC3_32c |
LR_STS33c_and_VC4_11c |
LR_STS34c_and_VC3_34c |
LR_STS35c_and_VC3_35c |
LR_STS36c_and_VC4_12c |
LR_STS37c_and_VC3_37c |
LR_STS38c_and_VC3_38c |
LR_STS39c_and_VC4_13c |
LR_STS40c_and_VC3_40c |
LR_STS41c_and_VC3_41c |
LR_STS42c_and_VC4_14c |
LR_STS43c_and_VC3_43c |
LR_STS44c_and_VC3_44c |
LR_STS45c_and_VC4_15c |
LR_STS46c_and_VC3_46c |
LR_STS47c_and_VC3_47c |
LR_STS48c_and_VC4_16c |
LR_STS49c_and_VC3_49c |
LR_STS50c_and_VC3_50c |
LR_STS51c_and_VC4_17c |
LR_STS52c_and_VC3_52c |
LR_STS53c_and_VC3_53c |
LR_STS54c_and_VC4_18c |
LR_STS55c_and_VC3_55c |
LR_STS56c_and_VC3_56c |
LR_STS57c_and_VC4_19c |
LR_STS58c_and_VC3_58c |
LR_STS59c_and_VC3_59c |
LR_STS60c_and_VC4_20c |
LR_STS61c_and_VC3_61c |
LR_STS62c_and_VC3_62c |
LR_STS63c_and_VC4_21c |
LR_STS64c_and_VC3_64c |
LR_STS65c_and_VC3_65c |
LR_STS66c_and_VC4_22c |
LR_STS67c_and_VC3_67c |
LR_STS68c_and_VC3_68c |
LR_STS69c_and_VC4_23c |
LR_STS70c_and_VC3_70c |
LR_STS71c_and_VC3_71c |
LR_STS72c_and_VC4_24c |
LR_STS73c_and_VC3_73c |
LR_STS74c_and_VC3_74c |
LR_STS75c_and_VC4_25c |
LR_STS76c_and_VC3_76c |
LR_STS77c_and_VC3_77c |
LR_STS78c_and_VC4_26c |
LR_STS79c_and_VC3_79c |
LR_STS80c_and_VC3_80c |
LR_STS81c_and_VC4_27c |
LR_STS82c_and_VC3_82c |
LR_STS83c_and_VC3_83c |
LR_STS84c_and_VC4_28c |
LR_STS85c_and_VC3_85c |
LR_STS86c_and_VC3_86c |
LR_STS87c_and_VC4_29c |
LR_STS88c_and_VC3_88c |
LR_STS89c_and_VC3_89c |
LR_STS90c_and_VC4_30c |
LR_STS91c_and_VC3_91c |
LR_STS92c_and_VC3_92c |
LR_STS93c_and_VC4_31c |
LR_STS94c_and_VC3_94c |
LR_STS95c_and_VC3_95c |
LR_STS96c_and_VC4_32c |
LR_STS97c_and_VC3_97c |
LR_STS98c_and_VC3_98c |
LR_STS99c_and_VC4_33c |
LR_STS100c_and_VC3_100c |
LR_STS101c_and_VC3_101c |
LR_STS102c_and_VC4_34c |
LR_STS103c_and_VC3_103c |
LR_STS104c_and_VC3_104c |
LR_STS105c_and_VC4_35c |
LR_STS106c_and_VC3_106c |
LR_STS107c_and_VC3_107c |
LR_STS108c_and_VC4_36c |
LR_STS109c_and_VC3_109c |
LR_STS110c_and_VC3_110c |
LR_STS111c_and_VC4_37c |
LR_STS112c_and_VC3_112c |
LR_STS113c_and_VC3_113c |
LR_STS114c_and_VC4_38c |
LR_STS115c_and_VC3_115c |
LR_STS116c_and_VC3_116c |
LR_STS117c_and_VC4_39c |
LR_STS118c_and_VC3_118c |
LR_STS119c_and_VC3_119c |
LR_STS120c_and_VC4_40c |
LR_STS121c_and_VC3_121c |
LR_STS122c_and_VC3_122c |
LR_STS123c_and_VC4_41c |
LR_STS124c_and_VC3_124c |
LR_STS125c_and_VC3_125c |
LR_STS126c_and_VC4_42c |
LR_STS127c_and_VC3_127c |
LR_STS128c_and_VC3_128c |
LR_STS129c_and_VC4_43c |
LR_STS130c_and_VC3_130c |
LR_STS131c_and_VC3_131c |
LR_STS132c_and_VC4_44c |
LR_STS133c_and_VC3_133c |
LR_STS134c_and_VC3_134c |
LR_STS135c_and_VC4_45c |
LR_STS136c_and_VC3_136c |
LR_STS137c_and_VC3_137c |
LR_STS138c_and_VC4_46c |
LR_STS139c_and_VC3_139c |
LR_STS140c_and_VC3_140c |
LR_STS141c_and_VC4_47c |
LR_STS142c_and_VC3_142c |
LR_STS143c_and_VC3_143c |
LR_STS144c_and_VC4_48c |
LR_STS145c_and_VC3_145c |
LR_STS146c_and_VC3_146c |
LR_STS147c_and_VC4_49c |
LR_STS148c_and_VC3_148c |
LR_STS149c_and_VC3_149c |
LR_STS150c_and_VC4_50c |
LR_STS151c_and_VC3_151c |
LR_STS152c_and_VC3_152c |
LR_STS153c_and_VC4_51c |
LR_STS154c_and_VC3_154c |
LR_STS155c_and_VC3_155c |
LR_STS156c_and_VC4_52c |
LR_STS157c_and_VC3_157c |
LR_STS158c_and_VC3_158c |
LR_STS159c_and_VC4_53c |
LR_STS160c_and_VC3_160c |
LR_STS161c_and_VC3_161c |
LR_STS162c_and_VC4_54c |
LR_STS163c_and_VC3_163c |
LR_STS164c_and_VC3_164c |
LR_STS165c_and_VC4_55c |
LR_STS166c_and_VC3_166c |
LR_STS167c_and_VC3_167c |
LR_STS168c_and_VC4_56c |
LR_STS169c_and_VC3_169c |
LR_STS170c_and_VC3_170c |
LR_STS171c_and_VC4_57c |
LR_STS172c_and_VC3_172c |
LR_STS173c_and_VC3_173c |
LR_STS174c_and_VC4_58c |
LR_STS175c_and_VC3_175c |
LR_STS176c_and_VC3_176c |
LR_STS177c_and_VC4_59c |
LR_STS178c_and_VC3_178c |
LR_STS179c_and_VC3_179c |
LR_STS180c_and_VC4_60c |
LR_STS181c_and_VC3_181c |
LR_STS182c_and_VC3_182c |
LR_STS183c_and_VC4_61c |
LR_STS184c_and_VC3_184c |
LR_STS185c_and_VC3_185c |
LR_STS186c_and_VC4_62c |
LR_STS187c_and_VC3_187c |
LR_STS188c_and_VC3_188c |
LR_STS189c_and_VC4_63c |
LR_STS190c_and_VC3_190c |
LR_STS191c_and_VC3_191c |
LR_STS192c_and_VC4_64c |
LR_STS768c_and_VC4_256c |
LR_T1_and_DS1_1_5M |
LR_T2_and_DS2_6M |
LR_T3_and_DS3_45M |
LR_VT1_5_and_TU11_VC11 |
LR_VT2_and_TU12_VC12 |
LR_VT6_and_TU2_VC2 |

XML
-<xsd:simpleType name="LayerRate_T"> -<xsd:annotation> <xsd:documentation> The LayerRate_T value is used to identify: - the Layer of a PTP/CTP, - the characteristic information of a PTP/FTP, - the Layer/Rate of a connection. Each LayerRate_T may be used in conjunction with a CTP/PTP/FTP of that layer. In the SDH definitions, the G.805 CP and G.805 Termination Function layer names differ, for example TU12 is used for the G.805 CP and VC12 for the corresponding G.805 Termination Function. In this interface definition the TU and VC definitions have been combined into a single composite layer and this has been named to include the equivalent SONET layer, e.g. LR_VT2_and_TU12_VC12. For more details refer to the following supporting document: - layering documentfor all layering concepts - LayerRates document for information about recognized values in MTOSI Any vendor extensions are permitted. However, they shall comply with MTOSI attribute vendor extension rule: Values must have the "PROP_" prefix. Refer to the TMF 854 XML Solution Set document for more details. </xsd:documentation> </xsd:annotation> -<xsd:union> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="PROP_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="LR_DS0_64K" /> <xsd:enumeration value="LR_DSL" /> <xsd:enumeration value="LR_Not_Applicable" /> <xsd:enumeration value="LR_Async_FOTS_150M" /> <xsd:enumeration value="LR_Async_FOTS_417M" /> <xsd:enumeration value="LR_Async_FOTS_560M" /> <xsd:enumeration value="LR_Async_FOTS_565M" /> <xsd:enumeration value="LR_Async_FOTS_1130M" /> <xsd:enumeration value="LR_Async_FOTS_1G7" /> <xsd:enumeration value="LR_Async_FOTS_1G8" /> <xsd:enumeration value="LR_ATM_NI" /> <xsd:enumeration value="LR_ATM_VC" /> <xsd:enumeration value="LR_ATM_VP" /> <xsd:enumeration value="LR_D1_Video" /> <xsd:enumeration value="LR_DIGITAL_SIGNAL_RATE" /> <xsd:enumeration value="LR_DIGITAL_SIGNAL_RATE" /> <xsd:enumeration value="LR_PHYSICAL_ELECTRICAL." /> <xsd:enumeration value="LR_DSR_1_5M" /> <xsd:enumeration value="LR_DSR_2M" /> <xsd:enumeration value="LR_DSR_4M" /> <xsd:enumeration value="LR_DSR_6M" /> <xsd:enumeration value="LR_DSR_8M" /> <xsd:enumeration value="LR_DSR_16M" /> <xsd:enumeration value="LR_DSR_34M" /> <xsd:enumeration value="LR_E2_8M" /> <xsd:enumeration value="LR_E5_565M" /> <xsd:enumeration value="LR_Encapsulation" /> <xsd:enumeration value="LR_Fragment" /> <xsd:enumeration value="LR_DSR_45M" /> <xsd:enumeration value="LR_DSR_140M" /> <xsd:enumeration value="LR_DSR_565M" /> <xsd:enumeration value="LR_DSR_Fast_Ethernet" /> <xsd:enumeration value="LR_DSR_Gigabit_Ethernet" /> <xsd:enumeration value="LR_DSR_10Gigabit_Ethernet" /> <xsd:enumeration value="LR_DSR_OC1_STM0" /> <xsd:enumeration value="LR_DSR_OC3_STM1" /> <xsd:enumeration value="LR_DSR_2xSTM1" /> <xsd:enumeration value="LR_DSR_OC12_STM4" /> <xsd:enumeration value="LR_DSR_OC24_STM8" /> <xsd:enumeration value="LR_DSR_OC48_and_STM16" /> <xsd:enumeration value="LR_DSR_OC192_and_STM64" /> <xsd:enumeration value="LR_DSR_OC768_and_STM256" /> <xsd:enumeration value="LR_DSR_OTU1" /> <xsd:enumeration value="LR_DSR_OTU2" /> <xsd:enumeration value="LR_DSR_OTU3" /> <xsd:enumeration value="LR_E1_2M" /> <xsd:enumeration value="LR_E20_2x2M" /> <xsd:enumeration value="LR_E30_8x2M" /> <xsd:enumeration value="LR_E3_34M" /> <xsd:enumeration value="LR_E4_140M" /> <xsd:enumeration value="LR_ESCON" /> <xsd:enumeration value="LR_Ethernet" /> <xsd:enumeration value="LR_ETR" /> <xsd:enumeration value="LR_Fast_Ethernet" /> <xsd:enumeration value="LR_FC_12_133M" /> <xsd:enumeration value="LR_FC_25_266M" /> <xsd:enumeration value="LR_FC_50_531M" /> <xsd:enumeration value="LR_FC_100_1063M" /> <xsd:enumeration value="LR_FDDI" /> <xsd:enumeration value="LR_FICON" /> <xsd:enumeration value="LR_FR_IF" /> <xsd:enumeration value="LR_FR_PVC" /> <xsd:enumeration value="LR_Gigabit_Ethernet" /> <xsd:enumeration value="LR_ISDN_BRI" /> <xsd:enumeration value="LR_Line_OC1_STS1_and_MS_STM0" /> <xsd:enumeration value="LR_Line_OC3_STS3_and_MS_STM1" /> <xsd:enumeration value="LR_Line_OC12_STS12_and_MS_STM4" /> <xsd:enumeration value="LR_Line_OC24_STS24_and_MS_STM8" /> <xsd:enumeration value="LR_Line_OC48_STS48_and_MS_STM16" /> <xsd:enumeration value="LR_Line_OC192_STS192_and_MS_STM64" /> <xsd:enumeration value="LR_Line_OC768_STS768_and_MS_STM256" /> <xsd:enumeration value="LR_Low_Order_TU3_VC3" /> <xsd:enumeration value="LR_OCH_Data_Unit_1" /> <xsd:enumeration value="LR_OCH_Data_Unit_2" /> <xsd:enumeration value="LR_OCH_Data_Unit_3" /> <xsd:enumeration value="LR_OCH_Transport_Unit_1" /> <xsd:enumeration value="LR_OCH_Transport_Unit_2" /> <xsd:enumeration value="LR_OCH_Transport_Unit_3" /> <xsd:enumeration value="LR_STS3c_and_AU4_VC4" /> <xsd:enumeration value="LR_STS4c_and_VC3_4c" /> <xsd:enumeration value="LR_STS5c_and_VC3_5c" /> <xsd:enumeration value="LR_STS6c_and_VC4_2c" /> <xsd:enumeration value="LR_STS7c_and_VC3_7c" /> <xsd:enumeration value="LR_STS8c_and_VC3_8c" /> <xsd:enumeration value="LR_STS9c_and_VC4_3c" /> <xsd:enumeration value="LR_Optical_Channel" /> <xsd:enumeration value="LR_Optical_Multiplex_Section" /> <xsd:enumeration value="LR_OPTICAL_SECTION" /> <xsd:enumeration value="LR_Optical_Transmission_Section" /> <xsd:enumeration value="LR_PHYSICAL_ELECTRICAL" /> <xsd:enumeration value="LR_PHYSICAL_MEDIALESS" /> <xsd:enumeration value="LR_PHYSICAL_OPTICAL" /> <xsd:enumeration value="LR_POTS" /> <xsd:enumeration value="LR_Section_OC1_STS1_and_RS_STM0" /> <xsd:enumeration value="LR_Section_OC3_STS3_and_RS_STM1" /> <xsd:enumeration value="LR_Section_OC12_STS12_and_RS_STM4" /> <xsd:enumeration value="LR_Section_OC24_STS24_and_RS_STM8" /> <xsd:enumeration value="LR_Section_OC48_STS48_and_RS_STM16" /> <xsd:enumeration value="LR_Section_OC192_STS192_and_RS_STM64" /> <xsd:enumeration value="LR_Section_OC768_STS768_and_RS_STM256" /> <xsd:enumeration value="LR_STS1_and_AU3_High_Order_VC3" /> <xsd:enumeration value="LR_STS2c_and_VC3_2c" /> <xsd:enumeration value="LR_STS10c_and_VC3_10c" /> <xsd:enumeration value="LR_STS11c_and_VC3_11c" /> <xsd:enumeration value="LR_STS12c_and_VC4_4c" /> <xsd:enumeration value="LR_STS13c_and_VC3_13c" /> <xsd:enumeration value="LR_STS14c_and_VC3_14c" /> <xsd:enumeration value="LR_STS15c_and_VC4_5c" /> <xsd:enumeration value="LR_STS16c_and_VC3_16c" /> <xsd:enumeration value="LR_STS17c_and_VC3_17c" /> <xsd:enumeration value="LR_STS18c_and_VC4_6c" /> <xsd:enumeration value="LR_STS19c_and_VC3_19c" /> <xsd:enumeration value="LR_STS20c_and_VC3_20c" /> <xsd:enumeration value="LR_STS21c_and_VC4_7c" /> <xsd:enumeration value="LR_STS22c_and_VC3_22c" /> <xsd:enumeration value="LR_STS23c_and_VC3_23c" /> <xsd:enumeration value="LR_STS24c_and_VC4_8c" /> <xsd:enumeration value="LR_STS25c_and_VC3_25c" /> <xsd:enumeration value="LR_STS26c_and_VC3_26c" /> <xsd:enumeration value="LR_STS27c_and_VC4_9c" /> <xsd:enumeration value="LR_STS28c_and_VC3_28c" /> <xsd:enumeration value="LR_STS29c_and_VC3_29c" /> <xsd:enumeration value="LR_STS30c_and_VC4_10c" /> <xsd:enumeration value="LR_STS31c_and_VC3_31c" /> <xsd:enumeration value="LR_STS32c_and_VC3_32c" /> <xsd:enumeration value="LR_STS33c_and_VC4_11c" /> <xsd:enumeration value="LR_STS34c_and_VC3_34c" /> <xsd:enumeration value="LR_STS35c_and_VC3_35c" /> <xsd:enumeration value="LR_STS36c_and_VC4_12c" /> <xsd:enumeration value="LR_STS37c_and_VC3_37c" /> <xsd:enumeration value="LR_STS38c_and_VC3_38c" /> <xsd:enumeration value="LR_STS39c_and_VC4_13c" /> <xsd:enumeration value="LR_STS40c_and_VC3_40c" /> <xsd:enumeration value="LR_STS41c_and_VC3_41c" /> <xsd:enumeration value="LR_STS42c_and_VC4_14c" /> <xsd:enumeration value="LR_STS43c_and_VC3_43c" /> <xsd:enumeration value="LR_STS44c_and_VC3_44c" /> <xsd:enumeration value="LR_STS45c_and_VC4_15c" /> <xsd:enumeration value="LR_STS46c_and_VC3_46c" /> <xsd:enumeration value="LR_STS47c_and_VC3_47c" /> <xsd:enumeration value="LR_STS48c_and_VC4_16c" /> <xsd:enumeration value="LR_STS49c_and_VC3_49c" /> <xsd:enumeration value="LR_STS50c_and_VC3_50c" /> <xsd:enumeration value="LR_STS51c_and_VC4_17c" /> <xsd:enumeration value="LR_STS52c_and_VC3_52c" /> <xsd:enumeration value="LR_STS53c_and_VC3_53c" /> <xsd:enumeration value="LR_STS54c_and_VC4_18c" /> <xsd:enumeration value="LR_STS55c_and_VC3_55c" /> <xsd:enumeration value="LR_STS56c_and_VC3_56c" /> <xsd:enumeration value="LR_STS57c_and_VC4_19c" /> <xsd:enumeration value="LR_STS58c_and_VC3_58c" /> <xsd:enumeration value="LR_STS59c_and_VC3_59c" /> <xsd:enumeration value="LR_STS60c_and_VC4_20c" /> <xsd:enumeration value="LR_STS61c_and_VC3_61c" /> <xsd:enumeration value="LR_STS62c_and_VC3_62c" /> <xsd:enumeration value="LR_STS63c_and_VC4_21c" /> <xsd:enumeration value="LR_STS64c_and_VC3_64c" /> <xsd:enumeration value="LR_STS65c_and_VC3_65c" /> <xsd:enumeration value="LR_STS66c_and_VC4_22c" /> <xsd:enumeration value="LR_STS67c_and_VC3_67c" /> <xsd:enumeration value="LR_STS68c_and_VC3_68c" /> <xsd:enumeration value="LR_STS69c_and_VC4_23c" /> <xsd:enumeration value="LR_STS70c_and_VC3_70c" /> <xsd:enumeration value="LR_STS71c_and_VC3_71c" /> <xsd:enumeration value="LR_STS72c_and_VC4_24c" /> <xsd:enumeration value="LR_STS73c_and_VC3_73c" /> <xsd:enumeration value="LR_STS74c_and_VC3_74c" /> <xsd:enumeration value="LR_STS75c_and_VC4_25c" /> <xsd:enumeration value="LR_STS76c_and_VC3_76c" /> <xsd:enumeration value="LR_STS77c_and_VC3_77c" /> <xsd:enumeration value="LR_STS78c_and_VC4_26c" /> <xsd:enumeration value="LR_STS79c_and_VC3_79c" /> <xsd:enumeration value="LR_STS80c_and_VC3_80c" /> <xsd:enumeration value="LR_STS81c_and_VC4_27c" /> <xsd:enumeration value="LR_STS82c_and_VC3_82c" /> <xsd:enumeration value="LR_STS83c_and_VC3_83c" /> <xsd:enumeration value="LR_STS84c_and_VC4_28c" /> <xsd:enumeration value="LR_STS85c_and_VC3_85c" /> <xsd:enumeration value="LR_STS86c_and_VC3_86c" /> <xsd:enumeration value="LR_STS87c_and_VC4_29c" /> <xsd:enumeration value="LR_STS88c_and_VC3_88c" /> <xsd:enumeration value="LR_STS89c_and_VC3_89c" /> <xsd:enumeration value="LR_STS90c_and_VC4_30c" /> <xsd:enumeration value="LR_STS91c_and_VC3_91c" /> <xsd:enumeration value="LR_STS92c_and_VC3_92c" /> <xsd:enumeration value="LR_STS93c_and_VC4_31c" /> <xsd:enumeration value="LR_STS94c_and_VC3_94c" /> <xsd:enumeration value="LR_STS95c_and_VC3_95c" /> <xsd:enumeration value="LR_STS96c_and_VC4_32c" /> <xsd:enumeration value="LR_STS97c_and_VC3_97c" /> <xsd:enumeration value="LR_STS98c_and_VC3_98c" /> <xsd:enumeration value="LR_STS99c_and_VC4_33c" /> <xsd:enumeration value="LR_STS100c_and_VC3_100c" /> <xsd:enumeration value="LR_STS101c_and_VC3_101c" /> <xsd:enumeration value="LR_STS102c_and_VC4_34c" /> <xsd:enumeration value="LR_STS103c_and_VC3_103c" /> <xsd:enumeration value="LR_STS104c_and_VC3_104c" /> <xsd:enumeration value="LR_STS105c_and_VC4_35c" /> <xsd:enumeration value="LR_STS106c_and_VC3_106c" /> <xsd:enumeration value="LR_STS107c_and_VC3_107c" /> <xsd:enumeration value="LR_STS108c_and_VC4_36c" /> <xsd:enumeration value="LR_STS109c_and_VC3_109c" /> <xsd:enumeration value="LR_STS110c_and_VC3_110c" /> <xsd:enumeration value="LR_STS111c_and_VC4_37c" /> <xsd:enumeration value="LR_STS112c_and_VC3_112c" /> <xsd:enumeration value="LR_STS113c_and_VC3_113c" /> <xsd:enumeration value="LR_STS114c_and_VC4_38c" /> <xsd:enumeration value="LR_STS115c_and_VC3_115c" /> <xsd:enumeration value="LR_STS116c_and_VC3_116c" /> <xsd:enumeration value="LR_STS117c_and_VC4_39c" /> <xsd:enumeration value="LR_STS118c_and_VC3_118c" /> <xsd:enumeration value="LR_STS119c_and_VC3_119c" /> <xsd:enumeration value="LR_STS120c_and_VC4_40c" /> <xsd:enumeration value="LR_STS121c_and_VC3_121c" /> <xsd:enumeration value="LR_STS122c_and_VC3_122c" /> <xsd:enumeration value="LR_STS123c_and_VC4_41c" /> <xsd:enumeration value="LR_STS124c_and_VC3_124c" /> <xsd:enumeration value="LR_STS125c_and_VC3_125c" /> <xsd:enumeration value="LR_STS126c_and_VC4_42c" /> <xsd:enumeration value="LR_STS127c_and_VC3_127c" /> <xsd:enumeration value="LR_STS128c_and_VC3_128c" /> <xsd:enumeration value="LR_STS129c_and_VC4_43c" /> <xsd:enumeration value="LR_STS130c_and_VC3_130c" /> <xsd:enumeration value="LR_STS131c_and_VC3_131c" /> <xsd:enumeration value="LR_STS132c_and_VC4_44c" /> <xsd:enumeration value="LR_STS133c_and_VC3_133c" /> <xsd:enumeration value="LR_STS134c_and_VC3_134c" /> <xsd:enumeration value="LR_STS135c_and_VC4_45c" /> <xsd:enumeration value="LR_STS136c_and_VC3_136c" /> <xsd:enumeration value="LR_STS137c_and_VC3_137c" /> <xsd:enumeration value="LR_STS138c_and_VC4_46c" /> <xsd:enumeration value="LR_STS139c_and_VC3_139c" /> <xsd:enumeration value="LR_STS140c_and_VC3_140c" /> <xsd:enumeration value="LR_STS141c_and_VC4_47c" /> <xsd:enumeration value="LR_STS142c_and_VC3_142c" /> <xsd:enumeration value="LR_STS143c_and_VC3_143c" /> <xsd:enumeration value="LR_STS144c_and_VC4_48c" /> <xsd:enumeration value="LR_STS145c_and_VC3_145c" /> <xsd:enumeration value="LR_STS146c_and_VC3_146c" /> <xsd:enumeration value="LR_STS147c_and_VC4_49c" /> <xsd:enumeration value="LR_STS148c_and_VC3_148c" /> <xsd:enumeration value="LR_STS149c_and_VC3_149c" /> <xsd:enumeration value="LR_STS150c_and_VC4_50c" /> <xsd:enumeration value="LR_STS151c_and_VC3_151c" /> <xsd:enumeration value="LR_STS152c_and_VC3_152c" /> <xsd:enumeration value="LR_STS153c_and_VC4_51c" /> <xsd:enumeration value="LR_STS154c_and_VC3_154c" /> <xsd:enumeration value="LR_STS155c_and_VC3_155c" /> <xsd:enumeration value="LR_STS156c_and_VC4_52c" /> <xsd:enumeration value="LR_STS157c_and_VC3_157c" /> <xsd:enumeration value="LR_STS158c_and_VC3_158c" /> <xsd:enumeration value="LR_STS159c_and_VC4_53c" /> <xsd:enumeration value="LR_STS160c_and_VC3_160c" /> <xsd:enumeration value="LR_STS161c_and_VC3_161c" /> <xsd:enumeration value="LR_STS162c_and_VC4_54c" /> <xsd:enumeration value="LR_STS163c_and_VC3_163c" /> <xsd:enumeration value="LR_STS164c_and_VC3_164c" /> <xsd:enumeration value="LR_STS165c_and_VC4_55c" /> <xsd:enumeration value="LR_STS166c_and_VC3_166c" /> <xsd:enumeration value="LR_STS167c_and_VC3_167c" /> <xsd:enumeration value="LR_STS168c_and_VC4_56c" /> <xsd:enumeration value="LR_STS169c_and_VC3_169c" /> <xsd:enumeration value="LR_STS170c_and_VC3_170c" /> <xsd:enumeration value="LR_STS171c_and_VC4_57c" /> <xsd:enumeration value="LR_STS172c_and_VC3_172c" /> <xsd:enumeration value="LR_STS173c_and_VC3_173c" /> <xsd:enumeration value="LR_STS174c_and_VC4_58c" /> <xsd:enumeration value="LR_STS175c_and_VC3_175c" /> <xsd:enumeration value="LR_STS176c_and_VC3_176c" /> <xsd:enumeration value="LR_STS177c_and_VC4_59c" /> <xsd:enumeration value="LR_STS178c_and_VC3_178c" /> <xsd:enumeration value="LR_STS179c_and_VC3_179c" /> <xsd:enumeration value="LR_STS180c_and_VC4_60c" /> <xsd:enumeration value="LR_STS181c_and_VC3_181c" /> <xsd:enumeration value="LR_STS182c_and_VC3_182c" /> <xsd:enumeration value="LR_STS183c_and_VC4_61c" /> <xsd:enumeration value="LR_STS184c_and_VC3_184c" /> <xsd:enumeration value="LR_STS185c_and_VC3_185c" /> <xsd:enumeration value="LR_STS186c_and_VC4_62c" /> <xsd:enumeration value="LR_STS187c_and_VC3_187c" /> <xsd:enumeration value="LR_STS188c_and_VC3_188c" /> <xsd:enumeration value="LR_STS189c_and_VC4_63c" /> <xsd:enumeration value="LR_STS190c_and_VC3_190c" /> <xsd:enumeration value="LR_STS191c_and_VC3_191c" /> <xsd:enumeration value="LR_STS192c_and_VC4_64c" /> <xsd:enumeration value="LR_STS768c_and_VC4_256c" /> <xsd:enumeration value="LR_T1_and_DS1_1_5M" /> <xsd:enumeration value="LR_T2_and_DS2_6M" /> <xsd:enumeration value="LR_T3_and_DS3_45M" /> <xsd:enumeration value="LR_VT1_5_and_TU11_VC11" /> <xsd:enumeration value="LR_VT2_and_TU12_VC12" /> <xsd:enumeration value="LR_VT6_and_TU2_VC2" /> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (8) Alarm_T/layerRate LayeredParameters_T/layer LayerRateList_T/layerRate ProtectionGroup_T/rate ProtectionSwitch_T/layerRate SubnetworkConnection_T/rate SwitchData_T/layerRate TopologicalLink_T/rate

Generated by WSDLdoc ©