Operation void getAllPTPNames (CIS SequenceOf Enums::LayerRate tpLayerRates = empty list, CIS SequenceOf Enums::LayerRate connectionLayerRates = empty list, CIS SequenceOf Name ptpNames = NA), in Class ManagedElement

Documentation
Get names of the PTPs that contain one or more of the NMS-specified TP layer rates and that are capable of containing CTPs that can be connected at one or more of the NMS-specified connection layer rates. This operation considers the capability/flexibility of the PTPs, not their current states.
The operation also returns FTPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when tpLayerRateList or connectionLayerRateList contain undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

tpLayerRates
/* in */ A list of TP Layer Rates used to scope the request. If the list is empty, all PTPs (of all rates) are returned.
connectionLayerRates
/* in */ The set of connection layer rates from which the reported PTPs must support at least one. If the list is empty then all PTPs (for all connection rates) are returned.
ptpNames
/* out */ A list of PTP names that are capable of supporting the provided TP and connection layer rates.