Operation void getBackupRoutes (Name routeId = NA, CIS Boolean includeHigherOrderCCs = False, CIS SequenceOf Structs::AVP additionalInfo = empty list, CIS SequenceOf Route routeList = empty list), in Class SubnetworkConnection

Documentation
This operation returns the specified route for the SNC. If the input route is not specified, the operation replies all the routes of the SNC, intended and backup ones. The rest of the behavior is the same as the getRoute() operation.
Note: The relationship between Bundled SNC service and the SNC with Multiple Routes feature requires further study and is not applicable for v3.0.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS does not implement the specified includeHigherOrderCCs value.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when any input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when routeId references an object that does not exist.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

routeId
/* in */ The identifier of the route.
includeHigherOrderCCs
/* in */ Specifies whether the higher order CCs of other SNCs used to carry the SNC route have to be included in addition to the CCs of the queried SNC route.
additionalInfo
/* inout */ Allows the communication of additional information which is not explicitly modelled.
routeList
/* out */ The route(s) of the SNC.